Risk assessment
Company name: Kestrel Build Ltd – Assessment carried out by: Martin Hale
Date assessment was carried out: 7 October 2026 – Date of next review: 7 January 2027
Risk Assessment Table
	What are the hazards?
	Who might be harmed and how?
	What are you already doing to control the risks?
	What further action do you need to take to control the risks?
	Who needs to carry out the action?
	When is the action needed by?
	Done

	Falls from scaffold and roof edge; falling materials from scaffold and roof work
	Roofers and labourers at risk of falls from the scaffold and roof edge; public on the shared driveway at risk from falling materials
	Independent tied scaffold erected by Avonside Scaffolding on 1 October; handover certificate on site; weekly inspection by MH. Edge protection and toe boards fitted.
	Brick guards on the top lift and a debris chute for the skip
	Martin Hale
	9 October 2026
	no

	Silica dust from disc cutter used for cutting blocks and paving
	Operatives breathing silica dust; neighbours' gardens downwind
	Cutter has a water suppression bottle; FFP3 masks issued and face-fit tested
	Hire an on-tool extraction saw for internal cutting
	Leanne Brooks (buyer)
	12 October 2026
	no

	Cement and lime handling — cement burns and dermatitis
	Labourers at risk of cement burns and dermatitis
	Gloves and goggles issued, washing facilities in the welfare unit
	No further action — existing controls are adequate
	Not applicable
	Not applicable
	yes

	Manual handling of block deliveries carried by hand to the rear
	Labourers at risk of back injuries
	Toolbox talk on lifting given on 5 October
	Hire a powered barrow and brief the team on lifting
	Martin Hale
	14 October 2026
	no


Further Information
More information on managing risk: www.hse.gov.uk/simple-health-safety/risk/
Published by the Health and Safety Executive 10/19
Published by the Health and Safety Executive 10/19    Page  of 
